IFC building model
Schema: "IFC4"
Description: "ViewDefinition [ReferenceView_V1.2]"
Description: "ExchangeRequirement [Structural]"
Description: "Option[Flat wide beams as plates:Off]"
Description: "Option[Location by:Global]"
Description: "Option[Locations from Organizer:On]"
Description: "Option[Layer:UDA[Name]]"
Description: "Option[Object coloring:ByObjectClass]"
Description: "Option[Export All:Off]"
Description: "Option[Export Pours:Off]"
File name: "SCAVALCO.ifc"
Time stamp: "2025-08-27T18:23:47"
Author: "fbercigli"
Organization: "Trimble"
Preprocessor: "Tekla Structures 2023 Service Pack 6"
Originating system: "IFC Export Version Sep 28 2023"
Authorization: "IFC4 test model"

Units
  LENGTHUNIT: MILLI METRE
  AREAUNIT: SQUARE_METRE
  VOLUMEUNIT: CUBIC_METRE
  MASSUNIT: KILO GRAM
  TIMEUNIT: SECOND
  PLANEANGLEUNIT: RADIAN
  SOLIDANGLEUNIT: STERADIAN
  THERMODYNAMICTEMPERATUREUNIT: DEGREE_CELSIUS
  LUMINOUSINTENSITYUNIT: LUMEN

Spatial structure
IFCPROJECT "Nome Progetto"
  IFCSITE "Unknown" | postal address: "Indirizzo"
    IFCBUILDING "Unknown" | postal address: "Indirizzo"
      contains 924 elements
        924 x IFCREINFORCINGBAR | names: "REBAR" | material: "B450C" | property sets: Pset_IdentificativoOggetto, Pset_ReinforcingBarCommon, Qto_ReinforcingElementBaseQuantities
      IFCBUILDINGSTOREY "Unknown" | elevation 0.
        contains 456 elements
          456 x IFCELEMENTASSEMBLY | names: "BAGGIOLO", "MURO PARAGHIAIA", "SPALLA" (+424 more) | parts: 518 IFCREINFORCINGBAR, 394 IFCBEAM, 40 IFCMECHANICALFASTENER, 32 IFCCOLUMN, 30 IFCPLATE | property sets: Pset_IdentificativoOggetto, Pset_ElementAssemblyCommon

Property sets
  Pset_IdentificativoOggetto | properties | on 1 object (1 IFCREINFORCINGBAR)
    Codice WBS = "016.011.058" (IFCLABEL)
    Codice elemento = "ARM" (IFCLABEL)
    ID elemento = "4a3815f3-2923-43a9-9b68-4ccfbf451f0c" (IFCLABEL)
  Pset_IdentificativoOggetto | properties | on 1 object (1 IFCREINFORCINGBAR)
    Codice WBS = "016.011.054" (IFCLABEL)
    Codice elemento = "ARM" (IFCLABEL)
    ID elemento = "1734b52b-0ea5-4d8d-8657-f27d4cf0027c" (IFCLABEL)
  Pset_IdentificativoOggetto | properties | on 1 object (1 IFCREINFORCINGBAR)
    Codice WBS = "016.011.058" (IFCLABEL)
    Codice elemento = "ARM" (IFCLABEL)
    ID elemento = "a3b1dd18-c580-47ff-b07b-271228717bc6" (IFCLABEL)
  Pset_IdentificativoOggetto | properties | on 1 object (1 IFCREINFORCINGBAR)
    Codice WBS = "016.011.058" (IFCLABEL)
    Codice elemento = "ARM" (IFCLABEL)
    ID elemento = "f2481f80-e821-481e-861b-2d78ba50c355" (IFCLABEL)
  Pset_IdentificativoOggetto | properties | on 1 object (1 IFCREINFORCINGBAR)
    Codice WBS = "016.011.054" (IFCLABEL)
    Codice elemento = "ARM" (IFCLABEL)
    ID elemento = "042cc18c-e56f-4c7a-bc25-e44eab2273da" (IFCLABEL)
  Pset_IdentificativoOggetto | properties | on 1 object (1 IFCREINFORCINGBAR)
    Codice WBS = "016.011.058" (IFCLABEL)
    Codice elemento = "ARM" (IFCLABEL)
    ID elemento = "07233365-35f4-4bf3-8d3e-4f396f63d651" (IFCLABEL)
  Pset_IdentificativoOggetto | properties | on 1 object (1 IFCREINFORCINGBAR)
    Codice WBS = "016.011.054" (IFCLABEL)
    Codice elemento = "ARM" (IFCLABEL)
    ID elemento = "784abbb3-e8d0-4eb1-8b67-0800b571d5d7" (IFCLABEL)
  Pset_IdentificativoOggetto | properties | on 1 object (1 IFCREINFORCINGBAR)
    Codice WBS = "016.011.058" (IFCLABEL)
    Codice elemento = "ARM" (IFCLABEL)
    ID elemento = "2237bfe0-4c04-40a5-803a-52725fb1d902" (IFCLABEL)
  Pset_IdentificativoOggetto: 2386 more contents on 2386 objects not shown
  Pset_ReinforcingBarCommon | properties | on 336 objects (336 IFCREINFORCINGBAR)
    BarLength = 8570. (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
    BendingShapeCode = "99" (IFCIDENTIFIER)
    NominalDiameter = 6. (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
    Reference = "D/4" (IFCIDENTIFIER)
    Status in {"NEW"} (IFCLABEL)
  Pset_ReinforcingBarCommon | properties | on 336 objects (336 IFCREINFORCINGBAR)
    BarLength = 5250. (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
    BendingShapeCode = "00" (IFCIDENTIFIER)
    NominalDiameter = 8. (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
    Reference = "TI/10" (IFCIDENTIFIER)
    Status in {"NEW"} (IFCLABEL)
  Pset_ReinforcingBarCommon | properties | on 168 objects (168 IFCREINFORCINGBAR)
    BarLength = 5250. (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
    BendingShapeCode = "00" (IFCIDENTIFIER)
    NominalDiameter = 10. (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
    Reference = "TS/11" (IFCIDENTIFIER)
    Status in {"NEW"} (IFCLABEL)
  Pset_ReinforcingBarCommon | properties | on 168 objects (168 IFCREINFORCINGBAR)
    BarLength = 3410. (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
    BendingShapeCode = "00" (IFCIDENTIFIER)
    NominalDiameter = 8. (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
    Reference = "TI/7" (IFCIDENTIFIER)
    Status in {"NEW"} (IFCLABEL)
  Pset_ReinforcingBarCommon | properties | on 168 objects (168 IFCREINFORCINGBAR)
    BarLength = 5550. (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
    BendingShapeCode = "99" (IFCIDENTIFIER)
    NominalDiameter = 6. (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
    Reference = "D/3" (IFCIDENTIFIER)
    Status in {"NEW"} (IFCLABEL)
  Pset_ReinforcingBarCommon | properties | on 84 objects (84 IFCREINFORCINGBAR)
    BarLength = 3410. (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
    BendingShapeCode = "00" (IFCIDENTIFIER)
    NominalDiameter = 10. (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
    Reference = "TS/12" (IFCIDENTIFIER)
    Status in {"NEW"} (IFCLABEL)
  Pset_ReinforcingBarCommon | properties | on 6 objects (6 IFCREINFORCINGBAR)
    BarLength = 3290. (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
    BarSpacing = 3. (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
    BendingShapeCode = "21" (IFCIDENTIFIER)
    NominalDiameter = 16. (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
    Reference = "ST/1" (IFCIDENTIFIER)
    Status in {"NEW"} (IFCLABEL)
  Pset_ReinforcingBarCommon | properties | on 6 objects (6 IFCREINFORCINGBAR)
    BarLength = 9020. (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
    BarSpacing = 1. (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
    BendingShapeCode = "11" (IFCIDENTIFIER)
    NominalDiameter = 16. (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
    Reference = "TS/10" (IFCIDENTIFIER)
    Status in {"NEW"} (IFCLABEL)
  Pset_ReinforcingBarCommon: 95 more contents on 170 objects not shown
  Qto_ReinforcingElementBaseQuantities | quantities | on 336 objects (336 IFCREINFORCINGBAR)
    Length = 8570. [MILLI METRE]
    Weight = 1.9 [KILO GRAM]
  Qto_ReinforcingElementBaseQuantities | quantities | on 336 objects (336 IFCREINFORCINGBAR)
    Length = 5250. [MILLI METRE]
    Weight = 2.07 [KILO GRAM]
  Qto_ReinforcingElementBaseQuantities | quantities | on 168 objects (168 IFCREINFORCINGBAR)
    Length = 5250. [MILLI METRE]
    Weight = 3.23 [KILO GRAM]
  Qto_ReinforcingElementBaseQuantities | quantities | on 168 objects (168 IFCREINFORCINGBAR)
    Length = 3410. [MILLI METRE]
    Weight = 1.35 [KILO GRAM]
  Qto_ReinforcingElementBaseQuantities | quantities | on 168 objects (168 IFCREINFORCINGBAR)
    Length = 5550. [MILLI METRE]
    Weight = 1.23 [KILO GRAM]
  Qto_ReinforcingElementBaseQuantities | quantities | on 84 objects (84 IFCREINFORCINGBAR)
    Length = 3410. [MILLI METRE]
    Weight = 2.1 [KILO GRAM]
  Qto_ReinforcingElementBaseQuantities | quantities | on 16 objects (16 IFCREINFORCINGBAR)
    Length = 12000. [MILLI METRE]
    Weight = 29.6 [KILO GRAM]
  Qto_ReinforcingElementBaseQuantities | quantities | on 16 objects (16 IFCREINFORCINGBAR)
    Length = 12000. [MILLI METRE]
    Weight = 18.9 [KILO GRAM]
  Qto_ReinforcingElementBaseQuantities: 46 more contents on 150 objects not shown
  Pset_ElementAssemblyCommon | properties | on 105 objects (105 IFCELEMENTASSEMBLY)
    Reference = "S/43" (IFCIDENTIFIER)
    Status in {"NEW"} (IFCLABEL)
  Pset_ElementAssemblyCommon | properties | on 63 objects (63 IFCELEMENTASSEMBLY)
    Reference = "S/44" (IFCIDENTIFIER)
    Status in {"NEW"} (IFCLABEL)
  Pset_ElementAssemblyCommon | properties | on 42 objects (42 IFCELEMENTASSEMBLY)
    Reference = "S/41" (IFCIDENTIFIER)
    Status in {"NEW"} (IFCLABEL)
  Pset_ElementAssemblyCommon | properties | on 38 objects (38 IFCELEMENTASSEMBLY)
    Reference = "P/4(?)" (IFCIDENTIFIER)
    Status in {"NEW"} (IFCLABEL)
  Pset_ElementAssemblyCommon | properties | on 21 objects (21 IFCELEMENTASSEMBLY)
    Reference = "S/45" (IFCIDENTIFIER)
    Status in {"NEW"} (IFCLABEL)
  Pset_ElementAssemblyCommon | properties | on 10 objects (10 IFCELEMENTASSEMBLY)
    Reference = "C/3" (IFCIDENTIFIER)
    Status in {"NEW"} (IFCLABEL)
  Pset_ElementAssemblyCommon | properties | on 10 objects (10 IFCELEMENTASSEMBLY)
    Reference = "A/1(?)" (IFCIDENTIFIER)
    Status in {"NEW"} (IFCLABEL)
  Pset_ElementAssemblyCommon | properties | on 10 objects (10 IFCELEMENTASSEMBLY)
    Reference = "A/2(?)" (IFCIDENTIFIER)
    Status in {"NEW"} (IFCLABEL)
  Pset_ElementAssemblyCommon: 48 more contents on 157 objects not shown
  Pset_BeamCommon | properties | on 332 objects (332 IFCBEAM)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    Roll = 0. (IFCPLANEANGLEMEASURE) [RADIAN]
    Slope = 1.5708 (IFCPLANEANGLEMEASURE) [RADIAN]
    Status in {"NEW"} (IFCLABEL)
  Pset_BeamCommon | properties | on 14 objects (14 IFCBEAM)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    Roll = 1.5708 (IFCPLANEANGLEMEASURE) [RADIAN]
    Slope = 0. (IFCPLANEANGLEMEASURE) [RADIAN]
    Status in {"NEW"} (IFCLABEL)
  Pset_BeamCommon | properties | on 10 objects (10 IFCBEAM)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    Roll = 0. (IFCPLANEANGLEMEASURE) [RADIAN]
    Slope = 1.57079 (IFCPLANEANGLEMEASURE) [RADIAN]
    Status in {"NEW"} (IFCLABEL)
  Pset_BeamCommon | properties | on 9 objects (9 IFCBEAM)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    Roll = 0. (IFCPLANEANGLEMEASURE) [RADIAN]
    Slope = 1.42173 (IFCPLANEANGLEMEASURE) [RADIAN]
    Status in {"NEW"} (IFCLABEL)
  Pset_BeamCommon | properties | on 4 objects (4 IFCBEAM)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    Roll = 0. (IFCPLANEANGLEMEASURE) [RADIAN]
    Slope = 0. (IFCPLANEANGLEMEASURE) [RADIAN]
    Status in {"NEW"} (IFCLABEL)
  Pset_BeamCommon | properties | on 4 objects (4 IFCBEAM)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    Roll = 1.57079 (IFCPLANEANGLEMEASURE) [RADIAN]
    Slope = 0. (IFCPLANEANGLEMEASURE) [RADIAN]
    Status in {"NEW"} (IFCLABEL)
  Pset_BeamCommon | properties | on 4 objects (4 IFCBEAM)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    Roll = 0. (IFCPLANEANGLEMEASURE) [RADIAN]
    Slope = 2.E-05 (IFCPLANEANGLEMEASURE) [RADIAN]
    Status in {"NEW"} (IFCLABEL)
  Pset_BeamCommon | properties | on 3 objects (3 IFCBEAM)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    Roll = 0. (IFCPLANEANGLEMEASURE) [RADIAN]
    Slope = 1.E-05 (IFCPLANEANGLEMEASURE) [RADIAN]
    Status in {"NEW"} (IFCLABEL)
  Pset_BeamCommon: 8 more contents on 14 objects not shown
  Qto_BeamBaseQuantities | quantities | on 105 objects (105 IFCBEAM)
    CrossSectionArea = 1.44 [SQUARE_METRE]
    GrossSurfaceArea = 0.05 [SQUARE_METRE]
    GrossVolume = 0.06 [CUBIC_METRE]
    GrossWeight = 144. [KILO GRAM]
    Length = 1000. [MILLI METRE]
    NetSurfaceArea = 2.63 [SQUARE_METRE]
    NetVolume = 0.06 [CUBIC_METRE]
    NetWeight = 144. [KILO GRAM]
    OuterSurfaceArea = 0.05 [SQUARE_METRE]
  Qto_BeamBaseQuantities | quantities | on 84 objects (84 IFCBEAM)
    CrossSectionArea = 1.44 [SQUARE_METRE]
    GrossSurfaceArea = 0.045 [SQUARE_METRE]
    GrossVolume = 0.054 [CUBIC_METRE]
    GrossWeight = 131. [KILO GRAM]
    Length = 908. [MILLI METRE]
    NetSurfaceArea = 2.39 [SQUARE_METRE]
    NetVolume = 0.054 [CUBIC_METRE]
    NetWeight = 131. [KILO GRAM]
    OuterSurfaceArea = 0.045 [SQUARE_METRE]
  Qto_BeamBaseQuantities | quantities | on 42 objects (42 IFCBEAM)
    CrossSectionArea = 1.44 [SQUARE_METRE]
    GrossSurfaceArea = 0.073 [SQUARE_METRE]
    GrossVolume = 0.087 [CUBIC_METRE]
    GrossWeight = 209. [KILO GRAM]
    Length = 1450. [MILLI METRE]
    NetSurfaceArea = 3.75 [SQUARE_METRE]
    NetVolume = 0.087 [CUBIC_METRE]
    NetWeight = 209. [KILO GRAM]
    OuterSurfaceArea = 0.073 [SQUARE_METRE]
  Qto_BeamBaseQuantities | quantities | on 38 objects (38 IFCBEAM)
    CrossSectionArea = 0.00092 [SQUARE_METRE]
    GrossSurfaceArea = 0.017 [SQUARE_METRE]
    GrossVolume = 0.00013 [CUBIC_METRE]
    GrossWeight = 1.01 [KILO GRAM]
    Length = 140. [MILLI METRE]
    NetSurfaceArea = 0.017 [SQUARE_METRE]
    NetVolume = 0.00013 [CUBIC_METRE]
    NetWeight = 1.01 [KILO GRAM]
    OuterSurfaceArea = 0.017 [SQUARE_METRE]
  Qto_BeamBaseQuantities | quantities | on 10 objects (10 IFCBEAM)
    CrossSectionArea = 0.0004 [SQUARE_METRE]
    GrossSurfaceArea = 0.588 [SQUARE_METRE]
    GrossVolume = 0.012 [CUBIC_METRE]
    GrossWeight = 92.3 [KILO GRAM]
    Length = 1130. [MILLI METRE]
    NetSurfaceArea = 1.24 [SQUARE_METRE]
    NetVolume = 0.012 [CUBIC_METRE]
    NetWeight = 92.3 [KILO GRAM]
    OuterSurfaceArea = 0.588 [SQUARE_METRE]
  Qto_BeamBaseQuantities | quantities | on 10 objects (10 IFCBEAM)
    CrossSectionArea = 0.25 [SQUARE_METRE]
    GrossSurfaceArea = 0.077 [SQUARE_METRE]
    GrossVolume = 0.039 [CUBIC_METRE]
    GrossWeight = 53.9 [KILO GRAM]
    Length = 1000. [MILLI METRE]
    NetSurfaceArea = 1.23 [SQUARE_METRE]
    NetVolume = 0.039 [CUBIC_METRE]
    NetWeight = 53.9 [KILO GRAM]
    OuterSurfaceArea = 0.077 [SQUARE_METRE]
  Qto_BeamBaseQuantities | quantities | on 10 objects (10 IFCBEAM)
    CrossSectionArea = 645. [SQUARE_METRE]
    GrossSurfaceArea = 0.014 [SQUARE_METRE]
    GrossVolume = 0.375 [CUBIC_METRE]
    GrossWeight = 899. [KILO GRAM]
    Length = 295. [MILLI METRE]
    NetSurfaceArea = 17.6 [SQUARE_METRE]
    NetVolume = 0.375 [CUBIC_METRE]
    NetWeight = 899. [KILO GRAM]
    OuterSurfaceArea = 0.014 [SQUARE_METRE]
  Qto_BeamBaseQuantities | quantities | on 10 objects (10 IFCBEAM)
    CrossSectionArea = 0.16 [SQUARE_METRE]
    GrossSurfaceArea = 1.5 [SQUARE_METRE]
    GrossVolume = 0.489 [CUBIC_METRE]
    GrossWeight = 1440. [KILO GRAM]
    Length = 1460. [MILLI METRE]
    NetSurfaceArea = 4.15 [SQUARE_METRE]
    NetVolume = 0.489 [CUBIC_METRE]
    NetWeight = 1170. [KILO GRAM]
    OuterSurfaceArea = 1.5 [SQUARE_METRE]
  Qto_BeamBaseQuantities: 27 more contents on 85 objects not shown
  Pset_ColumnCommon | properties | on 21 objects (21 IFCCOLUMN)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    Roll = 0. (IFCPLANEANGLEMEASURE) [RADIAN]
    Slope = 1.5708 (IFCPLANEANGLEMEASURE) [RADIAN]
    Status in {"NEW"} (IFCLABEL)
  Pset_ColumnCommon | properties | on 11 objects (11 IFCCOLUMN)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    Roll = 0. (IFCPLANEANGLEMEASURE) [RADIAN]
    Slope = 1.57079 (IFCPLANEANGLEMEASURE) [RADIAN]
    Status in {"NEW"} (IFCLABEL)
  Qto_ColumnBaseQuantities | quantities | on 11 objects (11 IFCCOLUMN)
    CrossSectionArea = 0.501 [SQUARE_METRE]
    GrossSurfaceArea = 51.2 [SQUARE_METRE]
    GrossVolume = 10. [CUBIC_METRE]
    GrossWeight = 24100. [KILO GRAM]
    Length = 20000. [MILLI METRE]
    NetSurfaceArea = 51.2 [SQUARE_METRE]
    NetVolume = 10. [CUBIC_METRE]
    NetWeight = 24100. [KILO GRAM]
    OuterSurfaceArea = 51.2 [SQUARE_METRE]
  Qto_ColumnBaseQuantities | quantities | on 11 objects (11 IFCCOLUMN)
    CrossSectionArea = 0.501 [SQUARE_METRE]
    GrossSurfaceArea = 61.3 [SQUARE_METRE]
    GrossVolume = 12. [CUBIC_METRE]
    GrossWeight = 28900. [KILO GRAM]
    Length = 24000. [MILLI METRE]
    NetSurfaceArea = 61.3 [SQUARE_METRE]
    NetVolume = 12. [CUBIC_METRE]
    NetWeight = 28900. [KILO GRAM]
    OuterSurfaceArea = 61.3 [SQUARE_METRE]
  Qto_ColumnBaseQuantities | quantities | on 10 objects (10 IFCCOLUMN)
    CrossSectionArea = 0.031 [SQUARE_METRE]
    GrossSurfaceArea = 0.206 [SQUARE_METRE]
    GrossVolume = 0.0071 [CUBIC_METRE]
    GrossWeight = 0. [KILO GRAM]
    Length = 230. [MILLI METRE]
    NetSurfaceArea = 0.206 [SQUARE_METRE]
    NetVolume = 0.0071 [CUBIC_METRE]
    NetWeight = 0. [KILO GRAM]
    OuterSurfaceArea = 0.206 [SQUARE_METRE]
  Pset_PlateCommon | properties | on 30 objects (30 IFCPLATE)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    Status in {"NEW"} (IFCLABEL)
  Qto_PlateBaseQuantities | quantities | on 10 objects (10 IFCPLATE)
    GrossArea = 0.16 [SQUARE_METRE]
    GrossVolume = 0.0032 [CUBIC_METRE]
    GrossWeight = 0. [KILO GRAM]
    NetArea = 0.352 [SQUARE_METRE]
    NetVolume = 0.0032 [CUBIC_METRE]
    NetWeight = 0. [KILO GRAM]
    Perimeter = 1600. [MILLI METRE]
    SideArea = 0.336 [SQUARE_METRE]
    Width = 20. [MILLI METRE]
  Qto_PlateBaseQuantities | quantities | on 10 objects (10 IFCPLATE)
    GrossArea = 0.09 [SQUARE_METRE]
    GrossVolume = 0.0027 [CUBIC_METRE]
    GrossWeight = 0. [KILO GRAM]
    NetArea = 0.216 [SQUARE_METRE]
    NetVolume = 0.0027 [CUBIC_METRE]
    NetWeight = 0. [KILO GRAM]
    Perimeter = 1200. [MILLI METRE]
    SideArea = 0.198 [SQUARE_METRE]
    Width = 30. [MILLI METRE]
  Qto_PlateBaseQuantities | quantities | on 10 objects (10 IFCPLATE)
    GrossArea = 0.09 [SQUARE_METRE]
    GrossVolume = 0.015 [CUBIC_METRE]
    GrossWeight = 0. [KILO GRAM]
    NetArea = 0.384 [SQUARE_METRE]
    NetVolume = 0.015 [CUBIC_METRE]
    NetWeight = 0. [KILO GRAM]
    Perimeter = 1200. [MILLI METRE]
    SideArea = 0.282 [SQUARE_METRE]
    Width = 170. [MILLI METRE]
  Pset_MechanicalFastenerCommon | properties | on 40 objects (40 IFCMECHANICALFASTENER)
    NominalDiameter = 10. (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
    NominalLength = 35. (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
  Pset_MechanicalFastenerBolt | properties | on 40 objects (40 IFCMECHANICALFASTENER)
    HeadShape = "Hexagon" (IFCLABEL)
    KeyShape = "Slot" (IFCLABEL)
    NutShape = "Hexagon" (IFCLABEL)
    NutsCount = 1 (IFCCOUNTMEASURE)
    ThreadDiameter = 10. (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
    ThreadLength = 35. (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
    WasherShape = "Standard" (IFCLABEL)
    WashersCount = 1 (IFCCOUNTMEASURE)